Не устанавливается IPSEC туннель между DFL-860e и DI-804HV и не только

Вкратце работает машина с Kerio в качестве шлюза. Был приобретен на замену DFL-860e  в качестве шлюза на двух провайдеров, vpn сервера для подключения двух офисов и кучи vpn-клиентов. Схема сети на данный момент такова:
Wan1: билайн на pppoe, адрес белый 212.х.х.х

Локальная сеть: 192.168.31.0
Wan2, DMZ не подключены
Пробовал Agressive mode, NAT Traversal (в примере он включен)

DFL:

	Model:

	DFL-860E


	System Time:

	04.06.13 03:13

	Uptime:

	0 days, 00:11:36 


	Configuration:

	Version 185


	Firmware Version:

	2.40.03.08-20375
Mar 11 2013



	


DI-804HV:
Firmware Version: V1.53RU, Wed, Apr 28 2010 
Device Time: Tue Jun 04 03:13:48 2013 

Проблема - не работает туннель, ошибки в логах следующие

DFL-806E

	2013-06-04
03:20:46
	Info
	IPSEC
1802708
	
	
	
	
	
	ike_sa_destroyed
ike_sa_killed

	ike_sa=" Initiator SPI ESP=0x2c8ab2c9, AH=0x1fab2bb2, IPComp=0xe34b685" 

	2013-06-04
03:20:46
	Notice
	IPSEC
1800105
	
	
	
	
	
	ike_delete_notification

	local_ip=212.x.x.x remote_ip=95.154.75.164 cookies=2c8ab2c91fab2bb2e34b685637e1b34c reason="Received delete notification" 

	2013-06-04
03:20:43
	Info
	IPSEC
1803024
	
	
	
	
	
	xauth_exchange_done

	statusmsg="Authentication failed" 

	2013-06-04
03:20:42
	Info
	IPSEC
1802703
	
	
	
	
	
	ike_sa_negotiation_completed
ike_sa_completed

	local_peer="212.x.x.x:4500 ID 212.x.x.x" remote_peer="95.154.75.164:4500 ID 10.x.x.x" initiator_spi="2c8ab2c9 1fab2bb2" responder_spi="e34b6856 37e1b34c" int_severity=6 

	2013-06-04
03:20:42
	Info
	IPSEC
1802024
	
	
	
	
	
	ike_sa_negotiation_completed

	options="Responder, NAT-T" mode="Main Mode" auth="XAUTH I pre-shared keys" encryption=des-cbc keysize= hash=sha1 dhgroup=2 bits=1024 lifetime=28800 

	2013-06-04
03:20:34
	Info
	IPSEC
1802708
	
	
	
	
	
	ike_sa_destroyed
ike_sa_killed

	ike_sa=" Initiator SPI ESP=0xb3415def, AH=0xe60a7382, IPComp=0x98bccef" 

	2013-06-04
03:20:34
	Notice
	IPSEC
1800105
	
	
	
	
	
	ike_delete_notification

	local_ip=212.x.x.x remote_ip=95.154.75.164 cookies=b3415defe60a738298bccef7e87108de reason="Received delete notification" 

	2013-06-04
03:20:31
	Info
	IPSEC
1803024
	
	
	
	
	
	xauth_exchange_done

	statusmsg="Authentication failed" 

	2013-06-04
03:20:30
	Info
	IPSEC
1802703
	
	
	
	
	
	ike_sa_negotiation_completed
ike_sa_completed

	local_peer="212.x.x.x:4500 ID 212.x.x.x" remote_peer="95.154.75.164:4500 ID 10.x.x.x" initiator_spi="b3415def e60a7382" responder_spi="98bccef7 e87108de" int_severity=6 

	2013-06-04
03:20:30
	Info
	IPSEC
1802024
	
	
	
	
	
	ike_sa_negotiation_completed

	options="Responder, NAT-T" mode="Main Mode" auth="XAUTH I pre-shared keys" encryption=des-cbc keysize= hash=sha1 dhgroup=2 bits=1024 lifetime=28800


DI-804HV


Tuesday June 04, 2013 03:20:29 receiving a re-Tx MM msg, response the last msg
Tuesday June 04, 2013 03:20:29 IKED re-TX : MM to 212.x.x.x
Tuesday June 04, 2013 03:20:29 receiving a re-Tx MM msg, response the last msg
Tuesday June 04, 2013 03:20:29 IKED re-TX : MM to 212.x.x.x
Tuesday June 04, 2013 03:20:29 Receive IKE M6(IDRESP) : 212.x.x.x --> 10.x.x.x
Tuesday June 04, 2013 03:20:29 IKE Phase1 (ISAKMP SA) established : 212.x.x.x <-> 10.x.x.x
Tuesday June 04, 2013 03:20:29 Receive XAUTH (REQUEST) : 212.x.x.x -> 10.x.x.x XAUTH type generic(0)
Tuesday June 04, 2013 03:20:29 Send XAUTH (REPLY) : 10.x.x.x -> 212.x.x.x username(testuser)
Tuesday June 04, 2013 03:20:30 Receve XAUTH (SET) : 212.x.x.x -> 10.x.x.x, auth faild
Tuesday June 04, 2013 03:20:30 Send XAUTH (ACK) : 10.x.x.x -> 212.x.x.x 

Настройки на DFL:

pre-shared key: testtest

ipsec interface:   local network    212.x.x.x



    remote network  all-nets



    encapsulation mode  tunnel



    все остальное в None



    IKE Algorithms:DES,SHA1 lifetime 28800 sec



    IPSEC Algorithms:DES,SHA1 lifetime 3600 sec 250000 kilobytes


Authentication pre-shared key testtest  


XAUTH off


IKE Settings Main DH group 2, PFS None, Per net, on if supported, use DPD


Keep alive disabled


dynamically add route on


add route off 

l2tp server:


inner ip address: 10.6.0.1


tunnel protocol:  l2tp


outer interface filter: ipsec interface


server ip: 212.x.x.x


ppp: use user authentication rules, флажки на всех MMPE, ip pool 10.0.6.10-10.0.6.100


allowed networks: all-nets

Local user database: ipsec_users  testuser testtest

User authentication rule:


agent: PPP


auth source: local


interface: l2tp server


originator IP: all-nets


terminator IP: 212.x.x.x


authentication options: local user db – ipsec_users


agent options:  use ms-chap (пробовал устанавливать все флаги — эффект тот же)


restrictions: idle time 1800, use multiple logins

IP rules

1 LAN  Allow  any  all-netsAddress: 0.0.0.0/0  lan  lannetAddress: 192.168.31.0/24  all_tcpudpicmpMembers: all_icmp, all_udp, all_tcp 

2  allow_ping_beeline_l2tp  Allow  l2tp-server  short_l2tp_poolAddress: 10.6.0.10-10.6.0.100  core  short_l2tp_serverAddress: 10.6.0.1  all_icmp 

3  allow_all_vpn_lan  Allow  l2tp-server  short_l2tp_poolAddress: 10.6.0.10-10.6.0.100  lan  lannetAddress: 192.168.31.0/24  all_tcpudpicmpMembers: all_icmp, all_udp, all_tcp 

4  allow_all_vpn_wan  Allow  l2tp-server  short_l2tp_poolAddress: 10.6.0.10-10.6.0.100  core  all-netsAddress: 0.0.0.0/0  all_tcpudpicmpMembers: all_icmp, all_udp, all_tcp 

5  allow_standard  NAT  lan  lannetAddress: 192.168.31.0/24  beeline  all-netsAddress: 0.0.0.0/0  all_tcpudpDestination ports: 0-65535 

6  drop_all_from_vpn  Drop  l2tp-server  short_l2tp_poolAddress: 10.6.0.10-10.6.0.100  any  all-netsAddress: 0.0.0.0/0  all_tcpudpDestination ports: 0-65535 

Route table:

1. Route IPv4  beeline  all-netsAddress: 0.0.0.0/0     80 No Direct route for network all-nets over interface b... 

2.  Route IPv4  wan1  wan1netAddress: 0.0.0.0/0     100 No Direct route for network wan1net over interface wa... 

3.  Route IPv4  lan  lannetAddress: 192.168.21.0/24     100 No Direct route for network lannet over interface lan... 
Настройки на DI-804HV
local subnet 192.168.33.0

local netmask 255.255.255.0

remote subnet 192.168.31.0

remote netmask 255.255.255.0

remote gateway 212.x.x.x

preshare key  testtest

xAUTH enabled

client mode on

user  testuser

password testtest

IPSEC NAT Traversal on
IKE Proporsal

DH Group 2, DES,SHA1, 28800 sec

IPSEC Proprosal

DH Group 2, ESP, DES,SHA1, 3600 sec
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