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Welcome To Hard Drive Configuration Wizard
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Step 1 :Physical Disk Information

subacture, th
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Step 2 :Select A RAID Type
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Step 2-2 :Auto-Rebuild Settings
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Step 4 :Volume Configuration Summary
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You are about to re-format the hard drive(s). All data will be
erased. Do you wish to continue?





Вариант 2 : Вставили новый HDD
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Welcome To Hard Drive Configuration Wizard
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Step 1 :Physical Disk Information
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Step 1 :Physical Disk Information
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Step 2 :Reconfigure the RAID Type to RAID 1
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Step 3 :Auto-Rebuild Settings
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Step 4 :Volume Configuration Summary





Итог имеем
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You are about to re-format the hard drive(s). All data will be
erased. Do you wish to continue?





