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D-Link

Building Networks for People DVG-5004S
FXS VolP Router

General Settings

Galler Filler Factory Default MAC Address 001E5842D848
Lanquage Net Link Connected

RIP Packet Summary Default Gateway 10.40.0.1
‘System Information DNS 10.40.0.1
Routing Table

STUN Inquiry
LAN PortInformation
Ping Test

Route Settings MAC Address 001E5842D849

System Setting

NTP

SNMP

Provision Seftings 1P Pool Range 192.168.8.1- 192.168.8.250
System Operation Lease Time 1 hour(s)

Logout DNS. 10.40.0.1

Driver Version 12.1.2168.14441242





