Please follow the steps to install:
1. Please copy the DGS-1224T folder and DGS-1248T to DevModule 
(Ex: Install the D-View in C:\Program Files, and copy the folders to C:\Program Files\D-Link\DevModule)
2. Choose Application——>Device Customization

3. Config the DGS-1224T as follow, then click the Apply button.
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Note:
Up Icon: C:\WINDOWS\system32\Resource\switch-on.bmp
Down Icon:C:\WINDOWS\system32\Resource\switch-off.bmp
Unpoll Icon:C:\WINDOWS\system32\Resource\switch-poll.bmp
Program: Choose the folder DGS-1224T’s DGS-1224TModule.exe
(Ex: If you follow the step 1’s example, then it be filled in
 C:\Program Files\D-Link\DevModule\DGS-1224T\DGS-1224TModule.exe)

4. Config the DGS-1248T as follow, then click the Apply button.
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Note:
Up Icon: C:\WINDOWS\system32\Resource\switch-on.bmp
Down Icon:C:\WINDOWS\system32\Resource\switch-off.bmp
Unpoll Icon:C:\WINDOWS\system32\Resource\switch-poll.bmp
Program: Choose the folder DGS-1248T’s DGS-1248TModule.exe
(Ex: If you follow the step 1’s example, then it be filled in
 C:\Program Files\D-Link\DevModule\DGS-1248T\DGS-1248TModule.exe)

